|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1. DEDE | DE | 12.7.2 |  | Ge | Readily available is not used in ECDIS context , see also corresponding requ for S-57 ENC in IEC 61174 Ed5 draft 5.3.3 | Replace  readily available  By  available on demand | I think this ok? If approved by group we can make this change. |
|  |  | 12.9.6 |  | Ge | Do we want/need to clarify how in route monitoring the highlights of the look-ahead area and the current and next route leg shall be combined, i.e. that these highlights shall not be additive and thus reduce readability | To be discussed | If this can be done and it’s not covered elsewhere this would be ok, would need a concrete proposal. Discuss at VTC (10/9/2025) |
|  |  | 12.9.10.3 | Figure 10 | Ge | Figure 10. shows the limitations of the algorithm.  On the upper side of the check area the CATZOC B area is partially covered by the smaller extension (20 m) | Discuss whether this solution is still considered to be good enough | Agree. Needs more discussion. Also there is input from ENCWG/S101PT to look at |
|  |  | 12.10.1 |  | Ge | Simple operator action is intended for general functions which are to be accessible from top level in 2 steps.  This is a nested function within another function (the legend) the term ‘simple operator action’ might be misleading in this case | Replace  … the suppressed information should be available through simple operator action, such as …  By  … the suppressed information should be easily accessible, e.g. by … | Discuss. |
|  |  | 12.10.3 | Table 4 | Te | The Note is misleading  If the (default 30 m or the selected) safety contour is not available, then the ECDIS shall use the next deeper safety contour.  There is always ONE safety contour | Remove the note on Value of safety contour | Clarify words. |
|  |  | 12.12.1 |  | te | Try to align display and filtering of NavWarnings as much as possible with existing equipment, e.g. NavTex or leave that to the OEM.  This is not the place to add new requirements to ECDIS that go beyond IMO PS and chart data product presentation | To be discussed | Discuss |
|  |  | 12.12.3 |  | te | Deviating from other data product, shall cancelled S-124 datasets really be kept for review.  For how long?  See also SevenCs comment on 12.13.3 of previous edition | To be discussed |  |
|  |  | 20.4.3 | a) iii | Ge | The note is unrelated | Remove note |  |
|  |  | Appendix D | D.2 | Ge | Readily available is not used in ECDIS context  See comment on 12.7.2 above | Replace  readily available  By available on demand | We can cover this alongside 12.7.2 |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |