|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| S-98 Main | SevenCs | 6.1.1 Basic product specifications and layers |  | ge | “…**must** be able to process and display at least the following data products:…”  “…the mariner must be able to switch the graphical display of S-111, S-124, S-129 on and off.”  The wording of the second requirement is ambiguous as it only refers to the display while the first requirement also refers to the processing. | “…the mariner must be able to switch processing and display of S-102, S-104, S-111, S-124, S-129 on and off. S-101, S-128 must always be enabled”.  The user selectors should be named and their effect should be defined unambiguously. | Discuss words. I don’t believe S-128 is always “enabled”. Agree we need to say it’s not just “display” but processing as well. Review words of para 6.1.1 again in VTC.  Look again when we draft Phase 2 requirement: |
|  |  | D-2 Water Level Adjustment (WLA) |  | ed | “The user must be able to **adjust depth information** by water level height in areas where both S-102 and S-104 data products are available.”  The wording implies user input for adjustment. | “The user must be able to **select** **depth information adjustment** by water level height in areas where both S-102 and S-104 data products are available.” | Agree. WE should make this edit. |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |